### Our Cloud Services and Features

### Additional DI/DO/AI

Customer can use for customization like cabinet side dg start fail alarms or temp sensor or Genset Remote Start

- 365Days History Log
- Real Time Regular Data Update 1min/3min/5min/10min
- Real Time onsite data can check in within 5sec
- Real Time Alarms
- Remote Engine Start/Stop/Reset Alarms
- Daily/Weekly/Monthly Energy Report in Excel
- Alarm Report in Excel Format
- Major and Minor Alarms
- Two Analog Input for fuel sensor/temp sensor
- Two digital input and output for external use
- Operator load current(A)/Consumption(Kwh)
- Two Battery Bank Charge/Discharge Current(A)
- Four Operator Supported

### Data Report Limitation

Users can able to export customized Reports in 50sheets

- Alarm In Dashboard/Email
- Abnormal Sensor alarms
- Genset Door Open Alarms
- Genset Manual Running Alarms
- Fuel Theft Alarms
- Device Offline Alarms
- Supported controller (DSE7320 AMF/MK2, SmartGen 9320 CAN)
- System Low Voltage Alarms(selectable under 48v)

### Cloud Server Limitation

Choosable cloud server package base on count of report sheets

- Difference User Access Level
- Unique Engine Control Interface base on Power Model
- Support both Desktop and Mobile
- Direct Site Access Control(Read only and Read-Write)

### Cost Saving

2.5G Network is enough coverage for any type of remote site location in Myanmar

- 365Days History Log
- Real Time Regular Data Update 1min/3min/5min/10min
- Real Time onsite data can check in within 5sec
- Real Time Alarms
- Remote Engine Start/Stop/Reset Alarms
- Daily/Weekly/Monthly Energy Report in Excel
- Alarm Report in Excel Format
- Major and Minor Alarms
- Operator load current(A)/Consumption(Kwh)
- Two Battery Bank Charge/Discharge Current(A)
- Four Operator Supported

### Data Report Limitation

Users can able to export customized Reports in 10 sheets

- Alarm In Dashboard/Email
- Abnormal Sensor alarms
- Genset Door Open Alarms
- Genset Manual Running Alarms
- Fuel Theft Alarms
- Cabinet Temperature Monitoring and High Temp Alarms
- Device Offline Alarms
- Supported controller (DSE7320 AMF/MK2, SmartGen 9320 CAN)
- System Low Voltage Alarms(selectable under 48v)

### Cloud Server Limitation

Choosable cloud server package base on count of report sheets

- Difference User Access Level
- Unique Engine Control Interface base on Power Model
- Support both Desktop and Mobile
- Direct Site Access Control(Individual site can check within one minute)

### Have a project in mind? Let’s get to work.

Contact Us